Commands on python:

* from: to import a library
* import: call a library
* camera: data type of camera library
* PiCamera(): used to access the camera
* Sleep(): wait for that many seconds

Libraries in raspberry:

* picamera
* time