LOG 5:

* Installed the vlc media player on the raspberry pi,

<https://thepi.io/how-to-compile-vlc-media-player-with-hardware-acceleration-for-the-raspberry-pi/>

* Followed it step by step on the terminal
* The second thing done was to setup the camera using python module <https://projects.raspberrypi.org/en/projects/getting-started-with-picamera/5>

In summary, was able to run .h264 videos on vlc media player after installing it on raspberry pi